MRTG-FAQ(1)                          mrtg                          MRTG-FAQ(1)



NNAAMMEE
       mrtg-faq - How to get help if you have problems with MRTG

SSYYNNOOPPSSIISS
       MRTG seems to raise a lot of questions. There are a number of resources
       apart from the documentation where you can find help for mrtg.

FFAAQQ
       In the following sections you'll find some additonal Frequently Asked
       Questions, with Answers.

       WWhhyy iiss tthheerree nnoo ""@@##$$%%"" ((mmyy nnaattiivvee llaanngguuaaggee)) vveerrssiioonn ooff MMRRTTGG??

       Nobody has contributed a _@_#_$_%_._p_m_d file yet. Go into the
       _m_r_t_g_-_2_._1_6_._2_/_t_r_a_n_s_l_a_t_e directory and create your own translation file.
       When you are happy with it send it to me for inclusion with the next
       mrtg release.

       II nneeeedd aa ssccrriipptt ttoo mmaakkee mmrrttgg wwoorrkk wwiitthh mmyy xxyyzz ddeevviiccee..

       Probably this has already been done. Check the stuff in the
       _m_r_t_g_-_2_._1_6_._2_/_c_o_n_t_r_i_b directory. There is a file called _0_0_I_N_D_E_X in that
       directory which tells what you can find in there.

       HHooww ddooeess tthhiiss SSNNMMPP tthhiinngg wwoorrkk

       There are many resources on the net that explain SNMP.  Take a look at
       this article from the Linux Journal by David Guerrero

        http://www.david-guerrero.com/papers/snmp/

       And at this rather long document from CISCO.

        http://www.cisco.com/univercd/cc/td/doc/cisintwk/ito_doc/snmp.htm

       TThhee iimmaaggeess ccrreeaatteedd bbyy MMRRTTGG llooookk vveerryy ssttrraannggee..

       Remove the *-{week,day,month,year}.png files and start MRTG again.
       Using MRTG for the first time, you might have to do this twice. This
       will also help when you introduce new routers into the cfg file.

       WWhhaatt iiss mmyy CCoommmmuunniittyy NNaammee??

       Ask the person in charge of your Router or try 'public', as this is the
       default Community Name.

       MMyy ggrraapphhss sshhooww aa ffllaatt lliinnee dduurriinngg aann oouuttaaggee.. WWhhyy ??

       Well, the short answer is that when an SNMP query goes out and a
       response doesn't come back, MRTG has to assume something to put in the
       graph, and by default it assumes that the last answer we got back is
       probably closer to the truth than zero.  This assumption is not perfect
       (as you have noticed).  It's a trade-off that happens to fail during a
       total outage.

       If this is an unacceptable trade-off, use the uunnkknnaasszzeerroo option.

       You may want to know what you're trading off, so in the spirit of
       trade-offs, here's the long answer:

       The problem is that MRTG doesn't know *why* the data didn't come back,
       all it knows is that it didn't come back.  It has to do something, and
       it assumes it's a stray lost packet rather than an outage.

       Why don't we always assume the circuit is down and use zero, which will
       (we think) be more nearly right?  Well, it turns out that you may be
       taking advantage of MRTG's "assume last" behaviour without being aware
       of it.

       MRTG uses SNMP (Simple Network Management Protocol) to collect data,
       and SNMP uses UDP (User Datagram Protocol) to ship packets around.  UDP
       is connectionless (not guaranteed) unlike TCP where packets are tracked
       and acknowledged and, if needed, retransmitted.  UDP just throws pack-
       ets at the network and hopes they arrive.  Sometimes they don't.

       One likely cause of lost SNMP data is congestion; another is busy
       routers.  Other possibilities include transient telecommunications
       problems, router buffer overflows (which may or may not be conges-
       tion-related), "dirty lines" (links with high error rates), and acts of
       God.  These things happen all the time; we just don't notice because
       many interactive services are TCP-based and the lost packets get
       retransmitted automatically.

       In the above cases where some SNMP packets are lost but traffic is
       flowing, assuming zero is the wrong thing to do - you end up with a
       graph that looks like it's missing teeth whenever the link fills up.
       MRTG interpolates the lost data to produce a smoother graph which is
       more accurate in cases of intermittent packet loss.  But with V2.8.4
       and above, you can use the "unknaszero" option to produce whichever
       graph is best under the conditions typical for your network.

AAUUTTHHOORR
       Tobias Oetiker <tobi@oetiker.ch>



2.16.2                            2008-05-16                       MRTG-FAQ(1)
