MRTG-MIBHELP(1)                      mrtg                      MRTG-MIBHELP(1)



NNAAMMEE
       mrtg-mibhelp - A Table of some interesting OIDs

OOVVEERRVVIIEEWW
       This File Contains a collection of interesting MIB Entries ...  mrtg
       knows about their names ... depending on the ASN.1 Syntax you may have
       to put ggaauuggee into the OOppttiioonnss[[]]:: parameter.

       For information about how to create a TTaarrggeett[[]]:: parameter which refer-
       ences these MIB entries, please consult mrtg-reference.

MMIIBB LLIISSTT
       iiffOOppeerrSSttaattuuss

        Descriptor:            ifOperStatus
        Identifier:            1.3.6.1.2.1.2.2.1.8
        ASN.1 Syntax:          INTEGER
        Enumeration:           up 1, down 2, testing 3

       The current operational state of the interface.  The _t_e_s_t_i_n_g(3) state
       indicates that no operational packets can be passed.

       iiffAAddmmiinnSSttaattuuss

        Descriptor:            ifAdminStatus
        Identifier:            1.3.6.1.2.1.2.2.1.7
        ASN.1 Syntax:          INTEGER
        Enumeration:           up 1, down 2, testing 3

       The current administrative state of the interface.  The _t_e_s_t_i_n_g(3)
       state indicates that no operational packets can be passed.

       iiffIInnOOcctteettss

        Descriptor:            ifInOctets
        Identifier:            1.3.6.1.2.1.2.2.1.10
        ASN.1 Syntax:          Counter32

       The total number of octets received on the interface, including framing
       characters.

       iiffIInnUUccaassttPPkkttss

        Descriptor:            ifInUcastPkts
        Identifier:            1.3.6.1.2.1.2.2.1.11
        ASN.1 Syntax:          Counter32

       The number of subnetwork-unicast packets delivered to a higher-layer
       protocol.

       iiffIInnNNUUccaassttPPkkttss

        Descriptor:            ifInNUcastPkts
        Identifier:            1.3.6.1.2.1.2.2.1.12
        ASN.1 Syntax:          Counter32

       The number of non-unicast (i.e., subnetwork- broadcast or subnet-
       work-multicast) packets delivered to a higher-layer protocol.

       iiffIInnDDiissccaarrddss

        Descriptor:            ifInDiscards
        Identifier:            1.3.6.1.2.1.2.2.1.13
        ASN.1 Syntax:          Counter32

       The number of inbound packets which were chosen to be discarded even
       though no errors had been detected to prevent their being deliverable
       to a higher-layer protocol.  One possible reason for discarding such a
       packet could be to free up buffer space.

       iiffIInnEErrrroorrss

        Descriptor:            ifInErrors
        Identifier:            1.3.6.1.2.1.2.2.1.14
        ASN.1 Syntax:          Counter32

       The number of inbound packets that contained errors preventing them
       from being deliverable to a higher-layer protocol.

       iiffIInnUUnnkknnoowwnnPPrroottooss

        Descriptor:            ifInUnknownProtos
        Identifier:            1.3.6.1.2.1.2.2.1.15
        ASN.1 Syntax:          Counter32

       The number of packets received via the interface which were discarded
       because of an unknown or unsupported protocol.

       iiffOOuuttOOcctteettss

        Descriptor:            ifOutOctets
        Identifier:            1.3.6.1.2.1.2.2.1.16
        ASN.1 Syntax:          Counter32

       The total number of octets transmitted out of the interface, including
       framing characters.

       iiffOOuuttUUccaassttPPkkttss

        Descriptor:            ifOutUcastPkts
        Identifier:            1.3.6.1.2.1.2.2.1.17
        ASN.1 Syntax:          Counter32

       The total number of packets that higher-level protocols requested be
       transmitted to a subnetwork-unicast address, including those that were
       discarded or not sent.

       iiffOOuuttNNUUccaassttPPkkttss

        Descriptor:             ifOutNUcastPkts
        Identifier:            1.3.6.1.2.1.2.2.1.18
        ASN.1 Syntax:          Counter32

       The total number of packets that higher-level protocols requested be
       transmitted to a non- unicast (i.e., a subnetwork-broadcast or subnet-
       work-multicast) address, including those that were discarded or not
       sent.

       iiffOOuuttDDiissccaarrddss

        Descriptor:             ifOutDiscards
        Identifier:            1.3.6.1.2.1.2.2.1.19
        ASN.1 Syntax:          Counter32

       The number of outbound packets which were chosen to be discarded even
       though no errors had been detected to prevent their being transmitted.
       One possible reason for discarding such a packet could be to free up
       buffer space.

       iiffOOuuttEErrrroorrss

        Descriptor:             ifOutErrors
        Identifier:            1.3.6.1.2.1.2.2.1.20
        ASN.1 Syntax:          Counter32

       The number of outbound packets that could not be transmitted because of
       errors.

       iiffOOuuttQQLLeenn

        Descriptor:             ifOutQLen
        Identifier:            1.3.6.1.2.1.2.2.1.21
        ASN.1 Syntax:          Unsigned32

       The length of the output packet queue (in packets).

       ffrrIInnOOcctteettss

       From: Simon Ferrett <simonf@world.net>

        'frInOctets' => '1.3.6.1.2.1.10.32.2.1.9'
        'frOutOctets' => '1.3.6.1.2.1.10.32.2.1.7'

       which when used in the form:

        frInOctets.pp.dd&frOutOctets.pp.dd:community@cisco.router

       where pp is the physical port that the frame relay pvc is defined on
       and dd is the DLCI of the pvc gets you the in and out octets for just
       that pvc.

       iiffAAddmmiinnHHaacckk aanndd iiffOOppeerrHHaacckk

       The return values of ifAdminStatus and ifOperStatus are not very use-
       full for graphing. Use ifOperHack and ifAdminHack instead. They return
       1 for UP and 0 otherwise.

       Note these are not real MIB entities but mrtg hacks

       PPsseeuuddooZZeerroo aanndd PPsseeuuddooOOnnee

       will return 0 and 1 respectively

       Note these are not real MIB entities but mrtg hacks

AAUUTTHHOORR
       Tobias Oetiker <tobi@oetiker.ch>



2.16.2                            2008-05-16                   MRTG-MIBHELP(1)
